Content

[2 Classes 1](#_Toc25400114)

[2.1 CurrentPerformance 1](#_Toc25400115)

[2.2 CurrentProblem 3](#_Toc25400116)

[2.3 HistoricalPerformance 4](#_Toc25400117)

[2.4 HybridMwStructureCapability 6](#_Toc25400118)

[2.5 HybridMwStructureConfiguration 7](#_Toc25400119)

[2.6 HybridMwStructureCurrentPerformance 9](#_Toc25400120)

[2.7 HybridMwStructureCurrentProblems 10](#_Toc25400121)

[2.8 HybridMwStructureHistoricalPerformances 10](#_Toc25400122)

[2.9 HybridMwStructureLpSpec 11](#_Toc25400123)

[2.10 HybridMwStructureStatus 12](#_Toc25400124)

[2.11 HybridMwStructure\_Pac 12](#_Toc25400125)

[2.12 TdmStructureKind 14](#_Toc25400126)

[3 Data Types 15](#_Toc25400127)

[3.1 G826ThresholdCrossAlarmType 15](#_Toc25400128)

[3.2 ProblemKindSeverityType 16](#_Toc25400129)

[3.3 SegmentStatusType 17](#_Toc25400130)

[3.4 StructureCurrentPerformanceType 18](#_Toc25400131)

[3.5 StructureCurrentProblemType 18](#_Toc25400132)

[3.6 StructureHistoricalPerformanceType 19](#_Toc25400133)

[3.7 StructurePerformanceType 19](#_Toc25400134)

[4 Enumeration Types 21](#_Toc25400135)

[4.1 AdministrativeStateType 21](#_Toc25400136)

[4.2 G826Type 22](#_Toc25400137)

[4.3 GranularityPeriodType 22](#_Toc25400138)

[4.4 LayerProtocolNameType 22](#_Toc25400139)

[4.5 OperationalStateType 22](#_Toc25400140)

[4.6 SeverityType 23](#_Toc25400141)

[5 Primitive Types 23](#_Toc25400142)

# Classes

## CurrentPerformance

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for CurrentPerformance

Table 1: Attributes for CurrentPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| timestamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | The timestamp associated with when the current data was collected. |
| suspectIntervalFlag | Boolean  false | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | This attribute is used to indicate that the performance data for the current period may not be reliable. Some reasons for this to occur are: – Suspect data were detected by the actual resource doing data collection. – Transition of the administrativeState attribute to/from the 'lock' state. – Transition of the operationalState to/from the 'disabled' state. – Scheduler setting that inhibits the collection function. – The performance counters were reset during the interval. – The currentData (or subclass) object instance was created during the monitoring period. |
| elapsedTime | Integer  -1 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: s  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_64\_BIT | Number of seconds that elapsed since the last reset of the counter. |
| scannerId | String  Scanner ID not defined. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| operationalState | OperationalStateType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| granularityPeriod | GranularityPeriodType  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Time period between reset of the underlying counter. |
| administrativeState | AdministrativeStateType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| objectClass | ObjectIdentifier  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | ObjectClass ::= CHOICE{ globalForm [0] OBJECT IDENTIFIER, localForm [1] INTEGER} |
| nameBinding | ObjectIdentifier  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| packages | ObjectIdentifier  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| allomorphs | ObjectIdentifier  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |

## CurrentProblem

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for CurrentProblem

Table 1: Attributes for CurrentProblem

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| sequenceNumber | Integer  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_16\_BIT | Unique sequence number of the current problem object. |
| timestamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Time when the alarm was raised. |
| problemSeverity | SeverityType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Severity of the alarm. |

## HistoricalPerformance

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for HistoricalPerformance

Table 1: Attributes for HistoricalPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| suspectIntervalFlag | Boolean  false | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | This attribute indicates that the data collected during the interval is suspect. |
| historyDataId | String  History Data ID not defined. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| periodEndTime | DateTime  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 2  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Time when the counter values have been recorded and the counter reset. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Time period between reset of the underlying counter. |
| objectClass | ObjectIdentifier  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | ObjectClass ::= CHOICE{ globalForm [0] OBJECT IDENTIFIER, localForm [1] INTEGER} |
| nameBinding | ObjectIdentifier  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| packages | ObjectIdentifier  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |
| allomorphs | ObjectIdentifier  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |

## HybridMwStructureCapability

Describes the logical structuring of the physical capacity provided by a hybrid microwave device (TDM + Ethernet). Segmentation is available. TDM transport is available.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureCapability

Table 1: Attributes for HybridMwStructureCapability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_supportedTdmStructureKindList | TdmStructureKind  ./. | 1..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Lists the TDM frame types that are supported. |
| supportedAlarmList | String  Supported alarms not yet defined. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Available alarms to be listed. Mandatory:none. Names are to be separated by commas. Further alarms might be added by the vendor. |
| performanceMonitoringIsAvail | Boolean  false | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | 1 = Collection and aggregation of performance values is available. |

## HybridMwStructureConfiguration

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureConfiguration

Table 1: Attributes for HybridMwStructureConfiguration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_tdmStructureKind | TdmStructureKind  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | TDM frame to be applied. |
| numberOfTdmSegmentsToBeReserved | Integer  -1 | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_8\_BIT | Allows to configure the number of segments reserved for TDM frames of the type specified in HybridMwStructure::HybridMwStructureConfiguration::structureType |
| problemKindSeverityList | ProblemKindSeverityType  ./. | 0..\* | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Severity of the type of problem to be configured. |
| g826ThresholdCrossAlarmList | G826ThresholdCrossAlarmType  ./. | 0..6 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | List of G826 related threshold cross alarms to be configured. |
| clearingThresholdCrossAlarmsIsOn | Boolean  false | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Setting this bit is clearing all the currently active threshold cross alarms. |
| performanceMonitoringIsOn | Boolean  false | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Enables measurement, collection, storage and access to performance data. |

## HybridMwStructureCurrentPerformance

Aggregated performance information of the structure of a hybrid microwave at a particular moment.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureCurrentPerformance

Table 1: Attributes for HybridMwStructureCurrentPerformance

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| currentPerformanceDataList | StructureCurrentPerformanceType  ./. | 1..2 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | At least values of the counters, which are reset every 15 minutes, are to be provided. If available, the current values of the counters, which are reset every 24 hour, can be provided, too. |

## HybridMwStructureCurrentProblems

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureCurrentProblems

Table 1: Attributes for HybridMwStructureCurrentProblems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| currentProblemList | StructureCurrentProblemType  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |

## HybridMwStructureHistoricalPerformances

Aggregated performance information of the structure of a hybrid microwave for a pre-defined measurement interval.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureHistoricalPerformances

Table 1: Attributes for HybridMwStructureHistoricalPerformances

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| historicalPerformanceDataList | StructureHistoricalPerformanceType  ./. | 0..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA |  |

## HybridMwStructureLpSpec

The HybridMwStructureLpSpec and its attached classes MUST be provided on management interfaces of microwave devices, which are transporting TDM and Ethernet traffic.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: YES
* objectDeletionNotification: YES
* OpenModelClass
* support: CONDITIONAL\_MANDATORY
* condition: hybrid-microwave

Attributes for HybridMwStructureLpSpec

Table 1: Attributes for HybridMwStructureLpSpec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_hybridMwStructure\_Pac | HybridMwStructure\_Pac  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |

## HybridMwStructureStatus

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructureStatus

Table 1: Attributes for HybridMwStructureStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| segmentStatusList | SegmentStatusType  ./. | 1..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Status of each segment (all TDM and one Ethernet). Multiplicity = HybridMwStructure::StructureConfiguration::tdmReservedNumberOfSegments + 1 |
| performanceMonitoringIsUp | Boolean  false | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | 1 = Performance values are currently collected and aggregated. |

## HybridMwStructure\_Pac

The HybridMwStructure\_Pac and its attached classes MUST be provided on management interfaces of microwave devices, which are transporting TDM and Ethernet traffic.

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for HybridMwStructure\_Pac

Table 1: Attributes for HybridMwStructure\_Pac

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_hybridMwStructureCapability | HybridMwStructureCapability  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_hybridMwStructureConfiguration | HybridMwStructureConfiguration  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_hybridMwStructureStatus | HybridMwStructureStatus  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_hybridMwStructureCurrentProblems | HybridMwStructureCurrentProblems  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_hybridMwStructureCurrentPerformance | HybridMwStructureCurrentPerformance  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_hybridMwStructureHistoricalPerformances | HybridMwStructureHistoricalPerformances  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |

## TdmStructureKind

Applied stereotypes:

* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* OpenModelClass
* support: MANDATORY

Attributes for TdmStructureKind

Table 1: Attributes for TdmStructureKind

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| tdmStructureName | String  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Names to be chosen from the following list: 'e1','t1','j1','e3','ds3','stm1','cpri1','cpri2','cpri3','cpri4','cpri5','cpri6' or 'cpri7' |
| tdmSegmentSize | Integer  -1 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kbit/s  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT | Size of the TDM segment in kbit/s. Values to be chosen from the following list: '2048','1544','34000','44736 ','155520','614400','1228800','2457600','3072000','4915200','6144000' or '9830400; |
| maxNumberOfSegmentsReservable | Integer  -1 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: segments  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_8\_BIT | Device specific maximum number of segments (not depending on current air interface configuration) that can be reserved for this type of segment on a single air interface. |

# Data Types

## G826ThresholdCrossAlarmType

Allows defining a threshold cross alarm.

Applied Stereotypes:

Attributes for G826ThresholdCrossAlarmType

Table 1: Attributes for G826ThresholdCrossAlarmType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| g826ValueKind | G826Type  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA | Kind of performance value that shall be equipped with a threshold alarm. |
| alarmRaisingThreshold | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_32\_BIT | Number of events required for raising the threshold cross alarm. |
| alarmClearingThreshold | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: LENGTH\_32\_BIT | Number of events required for clearing the threshold cross alarm. |
| granularityPeriod | GranularityPeriodType  NOT\_YET\_DEFINED | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA | Period of the performance data collection. |

## ProblemKindSeverityType

Applied Stereotypes:

Attributes for ProblemKindSeverityType

Table 1: Attributes for ProblemKindSeverityType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| problemKindName | String  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA | Name of the alarm according to supportedAlarmList |
| problemKindSeverity | SeverityType  NOT\_YET\_DEFINED | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA | Severity of this type of alarm. |

## SegmentStatusType

Applied Stereotypes:

Attributes for SegmentStatusType

Table 1: Attributes for SegmentStatusType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| segmentStatusTypeId | Integer  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_16\_BIT |  |
| segmentIsReservedForTdm | Boolean  false | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA | The number of segments, which is configured by Structure::StructureConfiguration::tdmReservedNumberOfSegements, has to be reserved for TDM. Starting from the lowest index value, these segments have to be marked with a 'true' in segmentIsReservedForTdm. |
| operationalStatus | OperationalStateType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: false * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: YES * bitLength: NA | Current operational status of each segment. |

## StructureCurrentPerformanceType

Turns performance information into current performance information by inheriting from OTN\_CurrentData.

Applied Stereotypes:

Attributes for StructureCurrentPerformanceType

Table 1: Attributes for StructureCurrentPerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| performanceData | StructurePerformanceType  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA |  |

## StructureCurrentProblemType

Applied Stereotypes:

Attributes for StructureCurrentProblemType

Table 1: Attributes for StructureCurrentProblemType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| problemName | String  Problem name not specified. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA | Name of the alarm according to Structure::StructureCapability::supportedAlarms |

## StructureHistoricalPerformanceType

Turns performance information into historical performance information by inheriting from OTN\_HistoryData.

Applied Stereotypes:

Attributes for StructureHistoricalPerformanceType

Table 1: Attributes for StructureHistoricalPerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| performanceData | StructurePerformanceType  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: no unit defined * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: NA |  |

## StructurePerformanceType

Consolidated performance information of the Structure.

Applied Stereotypes:

Attributes for StructurePerformanceType

Table 1: Attributes for StructurePerformanceType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| timePeriod | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT | Total length of the measurement period in seconds. |
| es | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT | Number of errored seconds. 1+0: Same value as for single air interface. 1+1 and Diversity: Value representing the combined signals. |
| ses | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT | Number of severely errored seconds. 1+0: Same value as for single air interface. 1+1 and Diversity: Value representing the combined signals. |
| cses | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT | Number of consecutive severely errored seconds. 1+0: Same value as for single air interface. 1+1 and Diversity: Value representing the combined signals. |
| unavailability | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: s * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_32\_BIT | Total time of unavailability in seconds. 1+0: Same value as for single air interface. 1+1 and Diversity: Value representing the combined signals. |
| rxLevelMin | Integer  99 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT | Minimum receive level. 1+0: Same value as for single air interface. 1+1: Value representing the combined signals. Diversity: To be left on default value. |
| rxLevelMax | Integer  99 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT | Maximum receive level. 1+0: Same value as for single air interface. 1+1: Value representing the combined signals. Diversity: To be left on default value. |
| rxLevelAvg | Integer  99 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * isInvariant: true * valueRange: no range constraint * unit: dBm * support: MANDATORY   OpenInterfaceModelAttribute   * AVC: NO * bitLength: LENGTH\_8\_BIT | Averaged receive level. 1+0: Same value as for single air interface. 1+1: Value representing the combined signals. Diversity: To be left on default value. |

# Enumeration Types

## AdministrativeStateType

For more information on Administrative State, See ITU-T Recs. X.731 and M.3100.

Contains Enumeration Literals:

* UNLOCKED:
* LOCKED:
* SHUTTING\_DOWN:
* NOT\_YET\_DEFINED:

## G826Type

Contains Enumeration Literals:

* ES:
  + Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::es .
* SES:
  + Severely Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::ses .
* CSES:
  + Consecutive Severely Errored Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::cses .
* UAS:
  + Unavailable Seconds. Threshold cross alarm will relate to TypeDefinitions::AirInterfacePerformanceType::unavailability.
* NOT\_SPECIFIED:

## GranularityPeriodType

The enumeration with the options for granularity period of the performance data.

Contains Enumeration Literals:

* UNKNOWN:
* PERIOD-15-MIN:
* PERIOD-24-HOURS:
* NOT\_YET\_DEFINED:

## LayerProtocolNameType

A controlled list of LayerProtocol names.

Contains Enumeration Literals:

* LAYER\_PROTOCOL\_NAME\_TYPE\_HYBRID\_MW\_STRUCTURE\_LAYER:

## OperationalStateType

The list of valid operational states for the connection.

Contains Enumeration Literals:

* ENABLED:
* DISABLED:
* NOT\_YET\_DEFINED:

## SeverityType

According to ITU-T M.3160

Contains Enumeration Literals:

* NON\_ALARMED:
* WARNING:
* MINOR:
* MAJOR:
* CRITICAL:
* NOT\_YET\_DEFINED:

# Primitive Types